CPVC

Submittal Information

PVC 45 Degree Elbow



|  |
| --- |
| * Standard Size Elbows Fabricated From Seamless

Extruded PVC Duct* All Fitting Dimensions Based on 1:1 Fitting Ratio
* Fitting Pieces Triple-Pass Welded Using 5/32”

PVC Welding Rod* All Dimensions in Inches
 |
|  |
| * All Dimensions are to CSSI standards and are

Subject to Change |

PRODUCT DIMENSIONS

|  |
| --- |
| 45 Degree Elbow-3 Pieces |

PVC 45 DEGREE ELBOW SUBMITTAL INFORMATION

45

Model Number Nominal Duct Size Average Duct O.D Average Wall Thickness End Type

|  |  |  |  |
| --- | --- | --- | --- |
|  |  |   |  |

|  |  |  |  |
| --- | --- | --- | --- |
|  45-PVC-6-1 | 6 | 6.625 | 0.187 |
|  45-PVC-7-1 | 7 | 7.375 | 0.187 |
|  45-PVC-8-1 | 8 | 8.625 | 0.187 |
|  45-PVC-9-1 | 9 | 9. 75 | 0.187 |
|  45-PVC-10-1 | 10 | 10.75 | 0.187 |
|  45-PVC-12-1 | 12 | 12.75 | 0.187 |
|  45-PVC-14-1 | 14 | 14 | 0.187 |
|  45-PVC-16-1 | 16 | 16 | 0.187 |
|  45-PVC-18-1 | 18 | 18 | 0.187 |
|  45-PVC-20-1 | 20 | 20 | 0.219 |
|  45-PVC-24-1 | 24 | 24 | 0.25 |

SOCKET

“B” END TYPE