PVC Reducer

F



Submitatal Information

|  |
| --- |
| * Custom Sized Reducers Available Upon Request * Constructed From I PVC Sheet for use in   Ventilation Systems   * All Dimensions in Inches |
|  |
| * All Dimensions are to CSSI standards and are   Subject to Change |

Note: if height is a concern please contact CSSI

PRODUCT DIMENSIONS

|  |
| --- |
|  |

**a**

PVC REDUCER SPECIFICATION CHART

SOCKET

Model Number Nominal Reducer Size A B End Type

|  |  |  |  |
| --- | --- | --- | --- |
| RE-PVC-6-4 | 6 TO 4 | 6.625 + 1/16 | 4.5 + 1/16 |
| RE-PVC-8-4 | 8 TO 4 | 8.625 + 1/16 | 4.5 + 1/16 |
| RE-PVC-8-6 | 8 TO 6 | 8.625 + 1/16 | 6.625 + 1/16 |
| RE-PVC-10-6 | 10 TO 6 | 10.75 + 1/16 | 6.625 + 1/16 |
| RE-PVC-10-8 | 10 TO 8 | 10.75 + 1/16 | 8.625 + 1/16 |
| RE-PVC-12-6 | 12 TO 6 | 12.75 + 1/16 | 6.625 + 1/16 |
| RE-PVC-12-8 | 12 TO 8 | 12.75 + 1/16 | 8.625 + 1/16 |
| RE-PVC-12-10 | 12 TO 10 | 12.75 + 1/16 | 10.75 + 1/16 |
| RE-PVC-14-6 | 14 TO 6 | 14 + 1/16 | 6.625 + 1/16 |
| RE-PVC-14-8 | 14 TO 8 | 14 + 1/16 | 8.625 + 1/16 |
| RE-PVC-14-10 | 14 TO 10 | 14 + 1/16 | 10.75 + 1/16 |
| RE-PVC-14-12 | 14 TO 12 | 14 + 1/16 | 12.75 + 1/16 |
| RE-PVC-16-8 | 16 TO 8 | 16 + 1/16 | 8.625 + 1/16 |
| RE-PVC-16-10 | 16 TO 10 | 16 + 1/16 | 10.75 + 1/16 |
| RE-PVC-16-12 | 16 TO 12 | 16 + 1/16 | 12.75 + 1/16 |
| RE-PVC-16-14 | 16 TO 14 | 16 + 1/16 | 14 + 1/16 |
| RE-PVC-18-8 | 18 TO 8 | 18 + 1/16 | 8.625 + 1/16 |
| RE-PVC-18-10 | 18 TO 10 | 18 + 1/16 | 10.75 + 1/16 |
| RE-PVC-18-12 | 18 TO 12 | 18 + 1/16 | 12.75 + 1/16 |
| RE-PVC-18-14 | 18 TO 14 | 18 + 1/16 | 14 + 1/16 |
| RE-PVC-18-16 | 18 TO 16 | 18 + 1/16 | 16 + 1/16 |
| RE-PVC-20-10 | 20 TO 10 | 20 + 1/16 | 10.75 + 1/16 |
| RE-PVC-20-12 | 20 TO 12 | 20 + 1/16 | 12.75 + 1/16 |
| RE-PVC-20-14 | 20 TO 14 | 20 + 1/16 | 14 + 1/16 |
| RE-PVC-20-16 | 20 TO 16 | 20 + 1/16 | 16 + 1/16 |
| RE-PVC-20-18 | 20 TO 18 | 20 + 1/16 | 18 + 1/16 |
| RE-PVC-24-12 | 24 TO 12 | 24 + 1/16 | 12.75 + 1/16 |
| RE-PVC-24-14 | 24 TO 14 | 24 + 1/16 | 14 + 1/16 |
| RE-PVC-24-16 | 24 TO 16 | 24 + 1/16 | 16 + 1/16 |
| RE-PVC-24-18 | 24 TO 18 | 24 + 1/16 | 18 + 1/16 |
| RE-PVC-24-20 | 24 TO 20 | 24 + 1/16 | 20 + 1/16 |

“B” END TYPE